**REMOTE CONTROL**

The remote control interface is shown as in Figure 2-7.



|  |  |  |
| --- | --- | --- |
| Button Number | Name | Same Function from the DVR Front Panel |
| 1 | Address | Press to input DVR serial number to enable user to control DVR. DVR Serial number will be the DVR address. |
| 2 | Multiple-window | Multiple windowswitch button as in the frontpanel labeled as (MULT) |
| 3 | 0-9 number key | Input password, channel or switch channel. Shift is the button to switch the input method. |
| 4 | Record | Used to control record function |
| 5 | Auxiliary key | 1. One-window monitor mode, click this button to display assistant function: PTZ control and image color.
2. Backspace function: in numeral control or text control, press it for 1.5 seconds to delete the previous character before the cursor.
3. In motion detection setup, working with Fn and direction keys to configure settings.
4. In text mode, click it to switch between numeral, English character(small/capitalized) and etc.
5. In HDD management interface, you can click it to switch HDD record information and other information
 |
| 6 | Confirm /menu | Used to confirm operation or go to MENU OSD |
| 7 | Cancel | 1. Go to previous menu, or cancel current operation
2. At playback screen: click it to restore real-time monitor mode
 |
| 8 | Direction | 1. Activate current control, modify setup, and then move up and down.
2. Increase or decrease numeral value
3. Function button for PTZ menu such as pan, tilt to left, right, up and downward.
4. Shift current activated control, and then move left and right
5. When at playback screen, click these buttons to control playback bar
 |
| 9 | Forward | Various forward speeds and normal speed playback. |
| 10 | Previous | In playback mode, playback the previous video. |
| 11 | Backward | In normal playback or pause mode, click this button toreverse Playback |
| 12 | Stop | Stops playback |