Port 554 needs to be port forwarded if the DVR will be accessed via Blackberry.

Blackberry is using RTSP protocol and needs port 554 to be open…… Jim B 3/17/2011